Raubfish builds:

 - Raubfisch X48e_nn_sl-64.exe for 64bit Windows systems
 - Raubfisch X48e_nn_sl-avx2.exe for 64-bit Windows systems and AMD processors
 - Raubfisch X48e_nn_sl-bmi2.exe for 64-bit Windows systems and Intel processors
 - Raubfisch X48e_nn_sl-general-64.exe for 64-bit general Windows systems
 - Raubfisch X48e_nn_sl-modern.exe for modern machines on a 64bit Windows system (uses popcnt asm-instruction)
 - Raubfisch X48e_nn_sl-sse3-popcnt.exe for machines using popcnt asm-instructions on a 64-bit Windows system having CPU Opteron (since Stepping E4), Sempron (since Palermo. Stepping E3), Athlon 64 (since Venice Stepping E3 and San Diego Stepping E4), Athlon 64 FX (since San Diego Stepping E4), Athlon 64 X2, Phenom 64 X2, Turion family, K10 family, APU family (including without GPU), FX Series, Zen, Zen+, Zen2, Celeron D, Celeron (starting with Core microarchitecture), Pentium 4 (since Prescott), Pentium D, Pentium Extreme Edition (but NOT Pentium 4 Extreme Edition), Pentium Dual-Core, Pentium (starting with Core microarchitecture), Intel Core, Intel Xeon (since Nocona), Intel Atom, VIA/Centaur C7, VIA/Centaur Nano, VIA/CentaurTransmeta Efficeon TM88xx (NOT Model Numbers TM86xx)

 - Raubfisch X48e_nn_sl-sse41-popcnt.exe for machines using popcnt asm-instructions on a 64-bit Windows system having CPU Intel Core 2 or AMD Bulldozer-based FX CPUs

 - Raubfisch X48e_nn_sl-ssse3.exe for 64-bit Windows system having CPU Opteron (since Stepping E4), Sempron (since Palermo. Stepping E3), Athlon 64 (since Venice Stepping E3 and San Diego Stepping E4), Athlon 64 FX (since San Diego Stepping E4), Athlon 64 X2, Phenom 64 X2, Turion family, K10 family, APU family (including without GPU), FX Series, Zen, Zen+, Zen2, Celeron D, Celeron (starting with Core microarchitecture), Pentium 4 (since Prescott), Pentium D, Pentium Extreme Edition (but NOT Pentium 4 Extreme Edition), Pentium Dual-Core, Pentium (starting with Core microarchitecture), Intel Core, Intel Xeon (since Nocona), Intel Atom, VIA/Centaur C7, VIA/Centaur Nano, VIA/CentaurTransmeta Efficeon TM88xx (NOT Model Numbers TM86xx)
